Stoichiometric AFR of Common Fuels:

Gasoline (pump fuel) - 14.7:1

Natural Gas - 17.2:1

Propane - 15.7:1

Ethanol - 9.0:1

E85 - 9.8:1

Methanol - 6.4:1

Diesel - 14.5:1